Note:

-b is command line parameter used to break the output as pages.

-? Is command line parameter used to display help about the command.

1. help -b: list all supported commands in UEFI shell.
2. memmap: Displays the memory map maintained by UEFI environment.
3. mm: Displays or modified MEM/MMIO/IO/PCI/PCIe address space.
4. mem: Displays the contents of system or device memory.
5. drivers -b: Displays the UEFI driver list.
6. devices: Display the list of devices supported by UEFI drivers.
7. devtree: Display the UEFI driver model complaint device tree.
8. bh -b: Displays the device handles associated with UEFI drivers.
9. dumpstore -all -b: Display the contents of the NVRAM variables.
10. stall: stalls the operation for a specified number of micro seconds.
11. load: Loads a UEFI driver